{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["废水排放"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"废水排放","index":0,"n_rows":70,"n_cols":22,"rows_kept":70,"merged":[[1,0,69,0],[1,1,17,1],[18,1,34,1],[35,1,51,1],[52,1,69,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","受纳水体","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","流量(m³/s)","水温(°C)","生产负荷(%)","进口浓度","排放浓度","上限","下限","单位","是否超标","超标倍数","备注","是否有评价限值"]
["2022年第4季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","废水处理设施出水口(WS-00099)","化学需氧量","2022-10-10",0,"22.6","","","7","40","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","总镉","2022-10-10",0,"22.6","","","<0.00005","0.01","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","石油类","2022-10-10",0,"22.6","","","<0.06","1","","mg/KG","否","","","是"]
["2022年第4季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","动植物油","2022-10-10",0,"22.6","","","<0.06","1","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","氨氮（NH3-N）","2022-10-10",0,"22.6","","","0.242","5;8","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","总汞","2022-10-10",0,"22.6","","","<0.00004","1","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","六价铬","2022-10-10",0,"22.6","","","<0.004","0.05","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","阴离子表面活性剂（LAS）","2022-10-10",0,"22.6","","","<0.05","0.5","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","总砷","2022-10-10",0,"22.6","","","0.00075","0.1","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","粪大肠菌群数","2022-10-10",0,"22.6","","","1000","1000","","个/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","pH值","2022-10-10",0,"22.6","","","7.7","9","6","无量纲","否","","","是"]
["2022年第4季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","总铅","2022-10-10",0,"22.6","","","<0.00009","0.1","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","悬浮物","2022-10-10",0,"22.6","","","10","10","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","总铬","2022-10-10",0,"22.6","","","<0.004","0.1","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","总氮（以N计）","2022-10-10",0,"22.6","","","1.50","15","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","废水处理设施出水口(WS-00099)","总磷（以P计）","2022-10-10",0,"22.6","","","0.02","0.5","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","紫金县古竹污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00099)","五日生化需氧量","2022-10-10",0,"22.6","","","1.3","10","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","五日生化需氧量","2022-10-12",0,"","","","1.4","4","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00061)","悬浮物","2022-10-12",0,"","","","<4","10","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00061)","总铬","2022-10-12",0,"","","","<0.004","0.1","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","镉","2022-10-12",0,"","","","<0.00005","0.005","","mg/KG","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","石油类","2022-10-12",0,"","","","<0.06","0.05","","mg/KG","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","汞","2022-10-12",0,"","","","<0.00004","0.0001","","mg/m3","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00061)","阴离子表面活性剂（LAS）","2022-10-12",0,"","","","<0.05","0.5","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","pH值","2022-10-12",0,"","","","7.4","9","6","无量纲","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00061)","六价铬","2022-10-12",0,"","","","<0.004","0.05","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00061)","动植物油","2022-10-12",0,"","","","<0.06","1","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","化学需氧量","2022-10-12",0,"","","","6","20","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","砷","2022-10-12",0,"","","","<0.00098","0.05","","mg/KG","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","铅","2022-10-12",0,"","","","<0.00009","0.05","","mg/Nm3","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(WS-00061)","氨氮（NH3-N）","2022-10-12",0,"","","","<0.025","1.0","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","总磷（以P计）","2022-10-12",0,"","","","<0.01","0.2","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施出水口(WS-00061)","粪大肠菌群数","2022-10-12",0,"","","","1500","10000","","个/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市广业环保有限公司河源市源城污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂水污染物排放标准(DB11/890-2012)(DB11/890-2012)","污水厂","废水处理设施出水口(WS-00061)","总氮（以N计）","2022-10-12",0,"","","","2.69","15","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施(DW001)","石油类","2022-11-01",0,"","","","<0.06","0.05","","mg/KG","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施(DW001)","砷","2022-11-01",0,"","","","0.00153","0.05","","mg/KG","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施(DW001)","汞","2022-11-01",0,"","","","<0.00004","0.0001","","mg/m3","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施(DW001)","氨氮（NH3-N）","2022-11-01",0,"","","","0.070","1.0","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施(DW001)","铅","2022-11-01",0,"","","","0.00054","0.05","","mg/Nm3","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施(DW001)","化学需氧量","2022-11-01",0,"","","","8","20","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施(DW001)","六价铬","2022-11-01",0,"","","","<0.004","0.05","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施(DW001)","阴离子表面活性剂（LAS）","2022-11-01",0,"","","","<0.05","0.2","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,三类,通用","废水处理设施(DW001)","五日生化需氧量","2022-11-01",0,"","","","<0.5","4","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施(DW001)","总镉","2022-11-01",0,"","","","<0.00005","0.005","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施(DW001)","动植物油","2022-11-01",0,"","","","<0.06","1","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施(DW001)","粪大肠菌群数","2022-11-01",0,"","","","1800","10000","","个/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施(DW001)","pH值","2022-11-01",0,"","","","7.7","9","6","无量纲","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施(DW001)","悬浮物","2022-11-01",0,"","","","10","10","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施(DW001)","总铬","2022-11-01",0,"","","","<0.004","0.1","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施(DW001)","总氮（以N计）","2022-11-01",0,"","","","6.19","15","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市市区城南污水处理厂","","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,2006年1月1日后建设","废水处理设施(DW001)","总磷（以P计）","2022-11-01",0,"","","","0.08","0.2","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,城镇二级污水处理厂","废水处理设施出水口(WS—00043)","化学需氧量","2022-11-02",0,"22.7","","","10","40","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水处理设施出水口(WS—00043)","总镉","2022-11-02",0,"22.7","","","<0.00005","0.01","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","石油类","2022-11-02",0,"22.7","","","<0.06","3","","mg/KG","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","动植物油","2022-11-02",0,"22.7","","","0.12","3","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","氨氮（NH3-N）","2022-11-02",0,"22.7","","","0.073","8;15","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水处理设施出水口(WS—00043)","总汞","2022-11-02",0,"22.7","","","<0.00004","0.001","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","化学需氧量","2022-11-02",0,"22.7","","","10","60","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水处理设施出水口(WS—00043)","六价铬","2022-11-02",0,"22.7","","","<0.004","0.05","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","阴离子表面活性剂（LAS）","2022-11-02",0,"22.7","","","<0.05","1","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水处理设施出水口(WS—00043)","总砷","2022-11-02",0,"22.7","","","0.00333","0.1","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","粪大肠菌群数","2022-11-02",0,"22.7","","","300","10000","","个/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","pH值","2022-11-02",0,"22.7","","","7.0","9","6","无量纲","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水处理设施出水口(WS—00043)","总铅","2022-11-02",0,"22.7","","","0.00138","0.1","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","悬浮物","2022-11-02",0,"22.7","","","10","20","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水处理设施出水口(WS—00043)","总铬","2022-11-02",0,"22.7","","","<0.004","0.1","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","总氮（以N计）","2022-11-02",0,"22.7","","","9.87","20","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,2005年12月31日前建设","废水处理设施出水口(WS—00043)","总磷（以P计）","2022-11-02",0,"22.7","","","1.09","1.5","","mg/L","否","","","是"]
["2022年第4季度重点污染源监督性监测","河源市污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理设施出水口(WS—00043)","五日生化需氧量","2022-11-02",0,"22.7","","","0.9","20","","mg/L","否","","","是"]