{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["废水排放","无组织","周边环境","厂界噪声"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"废水排放","index":0,"n_rows":35,"n_cols":22,"rows_kept":35,"merged":[[1,0,19,0],[1,1,19,1],[20,0,34,0],[20,1,34,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","受纳水体","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","流量(m³/s)","水温(°C)","生产负荷(%)","进口浓度","排放浓度","上限","下限","单位","是否超标","超标倍数","备注","是否有评价限值"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","出水口","总镉","2022-11-01",0,"","","","<0.001","0.01","","mg/L","否","","","是"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","出水口","石油类","2022-11-01",0,"","","","<0.06","1","","mg/L","否","","","是"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","出水口","动植物油","2022-11-01",0,"","","","0.06","1","","mg/L","否","","","是"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","出水口","氨氮（NH3-N）","2022-11-01",0,"","","","2.20","5","","mg/L","否","","","是"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","出水口","总汞","2022-11-01",0,"","","","<0.00002","0.001","","mg/L","否","","","是"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","出水口","色度","2022-11-01",0,"","","","5","30","","倍","否","","","是"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","出水口","烷基汞","2022-11-01",0,"","","","<0.000010","0","","mg/L","否","","","是"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","出水口","六价铬","2022-11-01",0,"","","","<0.004","0.05","","mg/L","否","","","是"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","出水口","阴离子表面活性剂（LAS）","2022-11-01",0,"","","","0.15","0.5","","mg/L","否","","","是"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","出水口","总砷","2022-11-01",0,"","","","0.0012","0.1","","mg/L","否","","","是"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","出水口","粪大肠菌群数","2022-11-01",0,"","","","330","1000","","个/L","否","","","是"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","出水口","pH值","2022-11-01",0,"","","","7.0","9","6","无量纲","否","","","是"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","出水口","总铅","2022-11-01",0,"","","","<0.1","0.1","","mg/L","否","","","是"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","出水口","悬浮物","2022-11-01",0,"","","","8","10","","mg/L","否","","","是"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","出水口","总铬","2022-11-01",0,"","","","<0.03","0.1","","mg/L","否","","","是"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","出水口","总氮（以N计）","2022-11-01",0,"","","","8.91","15","","mg/L","否","","","是"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","出水口","总磷（以P计）","2022-11-01",0,"","","","0.36","0.5","","mg/L","否","","","是"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","出水口","五日生化需氧量","2022-11-01",0,"","","","4.7","10","","mg/L","否","","","是"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","出水口","化学需氧量","2022-11-01",0,"","","","16","40","","mg/L","否","","","是"]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","废水排放口","六价铬","2022-10-16",0,"","","","<0.004","0.05","","mg/L","否","","","是"]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","废水排放口","色度","2022-10-16",0,"","","","<2","40","","倍","否","","","是"]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","","生活垃圾填埋污染控制标准(GB16889-2008)","表2标准","废水排放口","总氮","2022-10-16",0,"","","","0.75","40","","mg/L","否","","","是"]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","废水排放口","总铬","2022-10-16",0,"","","","<0.03","0.1","","mg/L","否","","","是"]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","废水排放口","粪大肠菌群数","2022-10-16",0,"","","","240","10000","","个/L","否","","","是"]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","废水排放口","总镉","2022-10-16",0,"","","","<0.001","0.01","","mg/L","否","","","是"]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","废水排放口","总铅","2022-10-16",0,"","","","<0.01","0.1","","mg/L","否","","","是"]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,一切排污单位","废水排放口","pH值","2022-10-16",0,"","","","6.5","9","6","无量纲","否","","","是"]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","废水排放口","化学需氧量","2022-10-16",0,"","","","16","90","","mg/L","否","","","是"]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","","水污染物排放限值标准（勿选）(DB44/26—2001)","表2 第二类污染物最高允许排放浓度,第一时段,一级标准","废水排放口","总磷（以P计）","2022-10-16",0,"","","","0.04","0.5","","mg/L","否","","","是"]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","废水排放口","悬浮物","2022-10-16",0,"","","","5","30","","mg/L","否","","","是"]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,其他排污单位","废水排放口","氨氮（NH3-N）","2022-10-16",0,"","","","<0.025","10","","mg/L","否","","","是"]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,天然橡胶乳加工、酒精、味精、皮革、化纤浆粕工业","废水排放口","五日生化需氧量","2022-10-16",0,"","","","3.8","20","","mg/L","否","","","是"]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","废水排放口","总砷","2022-10-16",0,"","","","<0.0003","0.1","","mg/L","否","","","是"]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","废水排放口","总汞","2022-10-16",0,"","","","<0.00004","0.001","","mg/L","否","","","是"]

{"sheet":"无组织","index":1,"n_rows":9,"n_cols":20,"rows_kept":9,"merged":[[1,0,8,0],[1,1,8,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","风向","风速（m/s）","温度(℃)","压力（kPa）","排放浓度","上限","下限","单位","是否超标","超标倍数","备注"]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","恶臭污染物排放标准(GB14554-93)","表1","上风向1#","臭气浓度","2022-10-16","","","","","<10","","","无量纲","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","恶臭污染物排放标准(GB14554-93)","表1","下风向3#","臭气浓度","2022-10-16","","","","","11","20","","无量纲","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值,直接排放","填埋区下风向4#","甲烷","2022-10-16","","","","","0.0012","0.1","","%","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值,直接排放","填埋区上风向1#","甲烷","2022-10-16","","","","","0.000465","","","%","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值,直接排放","填埋区下风向3#","甲烷","2022-10-16","","","","","0.00132","0.1","","%","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值,直接排放","填埋区下风向2#","甲烷","2022-10-16","","","","","0.00133","0.1","","%","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","恶臭污染物排放标准(GB14554-93)","表1","下风向2#","臭气浓度","2022-10-16","","","","","14","20","","无量纲","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","恶臭污染物排放标准(GB14554-93)","表1","下风向4#","臭气浓度","2022-10-16","","","","","12","20","","无量纲","否","",""]

{"sheet":"周边环境","index":2,"n_rows":24,"n_cols":35,"rows_kept":24,"merged":[[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,0,13],[0,14,0,17],[0,18,0,19],[0,20,0,24],[0,25,0,26],[0,27,1,27],[0,28,1,28],[0,29,1,29],[0,30,1,30],[0,31,1,31],[0,32,1,32],[0,33,1,33],[0,34,1,34],[2,0,23,0],[2,1,23,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","周边环境-环境空气","周边环境-环境空气","周边环境-环境空气","周边环境-环境空气","周边环境-环境空气","周边环境-地表水","周边环境-地表水","周边环境-地表水","周边环境-地表水","周边环境-地下水","周边环境-地下水","周边环境-土壤","周边环境-土壤","周边环境-土壤","周边环境-土壤","周边环境-土壤","周边环境-噪声","周边环境-噪声","折算/浓度/昼间","夜间","上限","下限","单位","是否超标","超标倍数","备注"]
["","","","","","","","","","湿度(%)","气温（℃","气压(kPa)","风速(m/s)","风向","流量(m³/s)","感官描述","有无漂浮物","有无油","井深（m）","水位（m）","采样深度(m)","土壤颜色","土壤水分(%)","利用情况","土壤pH值","声源","风速(m/s)","","","","","","","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","5#监测井","亚硝酸盐","2022-10-16","","","","","","","","","","","","","","","","","","","<0.001","","1.00","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","5#监测井","镉","2022-10-16","","","","","","","","","","","","","","","","","","","<0.0005","","0.005","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","5#监测井","氨氮","2022-10-16","","","","","","","","","","","","","","","","","","","0.38","","0.5","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅴ类","5#监测井","铜","2022-10-16","","","","","","","","","","","","","","","","","","","<0.009","","1.00","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","5#监测井","溶解性总固体","2022-10-16","","","","","","","","","","","","","","","","","","","46","","1000","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","5#监测井","铁","2022-10-16","","","","","","","","","","","","","","","","","","","0.0045","","0.3","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","5#监测井","砷","2022-10-16","","","","","","","","","","","","","","","","","","","<0.001","","0.01","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","5#监测井","挥发性酚类（以苯酚计）","2022-10-16","","","","","","","","","","","","","","","","","","","<0.002","","0.002","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅱ类","5#监测井","pH值","2022-10-16","","","","","","","","","","","","","","","","","","","6.54","","8.5","6.5","无量纲","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","5#监测井","氰化物","2022-10-16","","","","","","","","","","","","","","","","","","","<0.002","","0.05","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅴ类","5#监测井","六价铬","2022-10-16","","","","","","","","","","","","","","","","","","","<0.004","","0.05","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","5#监测井","硝酸盐（以N计）","2022-10-16","","","","","","","","","","","","","","","","","","","0.2","","20","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","5#监测井","锰","2022-10-16","","","","","","","","","","","","","","","","","","","0.0006","","0.10","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","5#监测井","总硬度","2022-10-16","","","","","","","","","","","","","","","","","","","23.7","","450","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","不评价/(不评价/)","不评价/","5#监测井","粪大肠菌群","2022-10-16","","","","","","","","","","","","","","","","","","","<20","","","","MPN/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","5#监测井","铅","2022-10-16","","","","","","","","","","","","","","","","","","","<0.0025","","0.01","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","5#监测井","汞","2022-10-16","","","","","","","","","","","","","","","","","","","<0.0001","","0.001","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","5#监测井","氯化物","2022-10-16","","","","","","","","","","","","","","","","","","","1.1","","250","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","","","5#监测井","高锰酸盐指数","2022-10-16","","","","","","","","","","","","","","","","","","","0.64","","3.0","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","5#监测井","锌","2022-10-16","","","","","","","","","","","","","","","","","","","0.03","","1.0","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","5#监测井","氟化物","2022-10-16","","","","","","","","","","","","","","","","","","","<0.2","","1.0","","mg/L","否","",""]
["2022年第四季度龙川县通衢镇老里塘垃圾综合填埋场监测","龙川县昱东环保科技有限公司","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","5#监测井","硫酸盐","2022-10-16","","","","","","","","","","","","","","","","","","","<5.0","","250","","mg/L","否","",""]

{"sheet":"厂界噪声","index":3,"n_rows":7,"n_cols":19,"rows_kept":7,"merged":[[1,0,6,0],[1,1,6,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","声源","风速（m/s）","昼间监测值","夜间监测值","上限","下限","单位","是否超标","超标倍数","备注"]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂东北","工业企业厂界环境噪声","2022-11-01","","","57","","65","","dB","否","",""]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂东南","工业企业厂界环境噪声","2022-11-01","","","58","","65","","dB","否","",""]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂西","工业企业厂界环境噪声","2022-11-01","","","56","","65","","dB","否","",""]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂南","工业企业厂界环境噪声","2022-11-01","","","58","","65","","dB","否","",""]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂东","工业企业厂界环境噪声","2022-11-01","","","56","","65","","dB","否","",""]
["2022年第四季度国控重点污染源监督性监测：龙川县城生活污水处理厂","河源市广业环保有限公司龙川县县城分公司","水环境","污水处理及其再生利用","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,3类厂界外声环境功能区,昼间/夜间","厂西南","工业企业厂界环境噪声","2022-11-01","","","57","","65","","dB","否","",""]