{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["废水排放","无组织","周边环境"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"废水排放","index":0,"n_rows":47,"n_cols":22,"rows_kept":47,"merged":[[1,0,46,0],[1,1,16,1],[17,1,46,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","受纳水体","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","流量(m³/s)","水温(°C)","生产负荷(%)","进口浓度","排放浓度","上限","下限","单位","是否超标","超标倍数","备注","是否有评价限值"]
["2023年东源县第一季度垃圾处理企业和污染源监测","河源市广业环保有限公司东源县城生活污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(1)","悬浮物","2023-03-13","","","","","8","10","","mg/L","否","","","是"]
["2023年东源县第一季度垃圾处理企业和污染源监测","河源市广业环保有限公司东源县城生活污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(1)","色度","2023-03-13","","","","","2","30","","倍","否","","","是"]
["2023年东源县第一季度垃圾处理企业和污染源监测","河源市广业环保有限公司东源县城生活污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,四类,通用","废水处理设施出水口(1)","阴离子表面活性剂（LAS）","2023-03-13","","","","","<0.05","0.3","","mg/L","否","","","是"]
["2023年东源县第一季度垃圾处理企业和污染源监测","河源市广业环保有限公司东源县城生活污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,四类,通用","废水处理设施出水口(1)","石油类","2023-03-13","","","","","<0.06","0.5","","mg/L","否","","","是"]
["2023年东源县第一季度垃圾处理企业和污染源监测","河源市广业环保有限公司东源县城生活污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,四类,通用","废水处理设施出水口(1)","总磷（以P计）","2023-03-13","","","","","0.24","0.3","","mg/L","否","","","是"]
["2023年东源县第一季度垃圾处理企业和污染源监测","河源市广业环保有限公司东源县城生活污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,四类,通用","废水处理设施出水口(1)","六价铬","2023-03-13","","","","","0.004","0.05","","mg/L","否","","","是"]
["2023年东源县第一季度垃圾处理企业和污染源监测","河源市广业环保有限公司东源县城生活污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(1)","pH值","2023-03-13","","","","","7.4","9","6","无量纲","否","","","是"]
["2023年东源县第一季度垃圾处理企业和污染源监测","河源市广业环保有限公司东源县城生活污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,四类,通用","废水处理设施出水口(1)","镉","2023-03-13","","","","","<0.00005","0.005","","mg/L","否","","","是"]
["2023年东源县第一季度垃圾处理企业和污染源监测","河源市广业环保有限公司东源县城生活污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,四类,通用","废水处理设施出水口(1)","铅","2023-03-13","","","","","<0.00009","0.05","","mg/L","否","","","是"]
["2023年东源县第一季度垃圾处理企业和污染源监测","河源市广业环保有限公司东源县城生活污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,四类,通用","废水处理设施出水口(1)","化学需氧量","2023-03-13","","","","","<10","30","","mg/L","否","","","是"]
["2023年东源县第一季度垃圾处理企业和污染源监测","河源市广业环保有限公司东源县城生活污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(1)","动植物油","2023-03-13","","","","","<0.06","1","","mg/L","否","","","是"]
["2023年东源县第一季度垃圾处理企业和污染源监测","河源市广业环保有限公司东源县城生活污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(1)","总氮（以N计）","2023-03-13","","","","","3.03","15","","mg/L","否","","","是"]
["2023年东源县第一季度垃圾处理企业和污染源监测","河源市广业环保有限公司东源县城生活污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水处理设施出水口(1)","粪大肠菌群数","2023-03-13","","","","","<10","1000","","个/L","否","","","是"]
["2023年东源县第一季度垃圾处理企业和污染源监测","河源市广业环保有限公司东源县城生活污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,四类,通用","废水处理设施出水口(1)","五日生化需氧量","2023-03-13","","","","","2.2","6","","mg/L","否","","","是"]
["2023年东源县第一季度垃圾处理企业和污染源监测","河源市广业环保有限公司东源县城生活污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,四类,通用","废水处理设施出水口(1)","氨氮（NH3-N）","2023-03-13","","","","","0.117","1.5","","mg/L","否","","","是"]
["2023年东源县第一季度垃圾处理企业和污染源监测","河源市广业环保有限公司东源县城生活污水处理厂","水环境","污水处理及其再生利用","","地表水环境质量标准(GB3838-2002)","表1地表水环境质量标准基本项目标准限值,四类,通用","废水处理设施出水口(1)","砷","2023-03-13","","","","","0.00097","0.1","","mg/L","否","","","是"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口2#(DW001)","悬浮物","2023-03-21","","","","","4","30","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口2#(DW001)","粪大肠菌群数","2023-03-21","","","","","1700","10000","","个/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","","","污水处理设施排放口2#(DW001)","pH值","2023-03-21","","","","","6.1","","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口2#(DW001)","氨氮（NH3-N）","2023-03-21","","","","","1.52","25","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口2#(DW001)","总氮（以N计）","2023-03-21","","","","","20.8","40","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口2#(DW001)","五日生化需氧量","2023-03-21","","","","","5.5","30","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口2#(DW001)","总汞","2023-03-21","","","","","<0.00004","0.001","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口2#(DW001)","总铬","2023-03-21","","","","","0.010","0.1","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口2#(DW001)","化学需氧量","2023-03-21","","","","","23","100","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口2#(DW001)","总铅","2023-03-21","","","","","<0.05","0.1","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口2#(DW001)","总镉","2023-03-21","","","","","<0.01","0.01","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口2#(DW001)","总磷（以P计）","2023-03-21","","","","","0.02","3","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口2#(DW001)","总砷","2023-03-21","","","","","0.0012","0.1","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口2#(DW001)","六价铬","2023-03-21","","","","","<0.004","0.05","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口2#(DW001)","色度","2023-03-21","","","","","2","40","","倍","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口1#(DW002)","五日生化需氧量","2023-03-21","","","","","1.4","30","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口1#(DW002)","总汞","2023-03-21","","","","","<0.00004","0.001","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口1#(DW002)","总铅","2023-03-21","","","","","<0.05","0.1","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口1#(DW002)","总镉","2023-03-21","","","","","<0.01","0.01","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口1#(DW002)","总氮（以N计）","2023-03-21","","","","","142","40","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","","","污水处理设施排放口1#(DW002)","pH值","2023-03-21","","","","","5.1","","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口1#(DW002)","总砷","2023-03-21","","","","","0.0016","0.1","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口1#(DW002)","氨氮（NH3-N）","2023-03-21","","","","","51.6","25","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口1#(DW002)","悬浮物","2023-03-21","","","","","8","30","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口1#(DW002)","总磷（以P计）","2023-03-21","","","","","0.05","3","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口1#(DW002)","化学需氧量","2023-03-21","","","","","6","100","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口1#(DW002)","总铬","2023-03-21","","","","","0.011","0.1","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口1#(DW002)","色度","2023-03-21","","","","","2","40","","倍","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口1#(DW002)","六价铬","2023-03-21","","","","","<0.004","0.05","","mg/L","否","","不外排,用于浇灌场区绿化","否"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","污水处理设施排放口1#(DW002)","粪大肠菌群数","2023-03-21","","","","","400","10000","","个/L","否","","不外排,用于浇灌场区绿化","否"]

{"sheet":"无组织","index":1,"n_rows":9,"n_cols":20,"rows_kept":9,"merged":[[1,0,8,0],[1,1,8,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","风向","风速（m/s）","温度(℃)","压力（kPa）","排放浓度","上限","下限","单位","是否超标","超标倍数","备注"]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值,直接排放","西侧场界外1米3#","甲烷","2023-03-21","","","","","0.000223","0.1","","%","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","西侧场界外1米3#","臭气浓度","2023-03-21","","","","","18","20","","无量纲","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值,直接排放","北侧场界外1米4#","甲烷","2023-03-21","","","","","0.000282","0.1","","%","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","北侧场界外1米4#","臭气浓度","2023-03-21","","","","","42","20","","无量纲","是","1.10",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值,直接排放","南侧场界外1米2#","甲烷","2023-03-21","","","","","0.000232","0.1","","%","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","南侧场界外1米2#","臭气浓度","2023-03-21","","","","","16","20","","无量纲","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","东侧场界外1米1#","臭气浓度","2023-03-21","","","","","46","20","","无量纲","是","1.30",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值,直接排放","东侧场界外1米1#","甲烷","2023-03-21","","","","","0.00195","0.1","","%","否","",""]

{"sheet":"周边环境","index":2,"n_rows":90,"n_cols":35,"rows_kept":90,"merged":[[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,0,13],[0,14,0,17],[0,18,0,19],[0,20,0,24],[0,25,0,26],[0,27,1,27],[0,28,1,28],[0,29,1,29],[0,30,1,30],[0,31,1,31],[0,32,1,32],[0,33,1,33],[0,34,1,34],[2,0,89,0],[2,1,89,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","周边环境-环境空气","周边环境-环境空气","周边环境-环境空气","周边环境-环境空气","周边环境-环境空气","周边环境-地表水","周边环境-地表水","周边环境-地表水","周边环境-地表水","周边环境-地下水","周边环境-地下水","周边环境-土壤","周边环境-土壤","周边环境-土壤","周边环境-土壤","周边环境-土壤","周边环境-噪声","周边环境-噪声","折算/浓度/昼间","夜间","上限","下限","单位","是否超标","超标倍数","备注"]
["","","","","","","","","","湿度(%)","气温（℃","气压(kPa)","风速(m/s)","风向","流量(m³/s)","感官描述","有无漂浮物","有无油","井深（m）","水位（m）","采样深度(m)","土壤颜色","土壤水分(%)","利用情况","土壤pH值","声源","风速(m/s)","","","","","","","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","氟化物","2023-03-21","","","","","","","","","","","","","","","","","","","0.24","","1.0","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","氨氮","2023-03-21","","","","","","","","","","","","","","","","","","","0.434","","0.5","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","铁","2023-03-21","","","","","","","","","","","","","","","","","","","<0.03","","0.3","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","铅","2023-03-21","","","","","","","","","","","","","","","","","","","<0.001","","0.01","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","pH值","2023-03-21","","","","","","","","","","","","","","","","","","","6.0","","8.5","6.5","无量纲","是","/",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","硝酸盐（以N计）","2023-03-21","","","","","","","","","","","","","","","","","","","0.05","","20.0","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","总硬度","2023-03-21","","","","","","","","","","","","","","","","","","","<5","","450","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","溶解性总固体","2023-03-21","","","","","","","","","","","","","","","","","","","151","","1000","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","铬（六价）","2023-03-21","","","","","","","","","","","","","","","","","","","<0.004","","0.05","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","锰","2023-03-21","","","","","","","","","","","","","","","","","","","<0.01","","0.10","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","硫酸盐","2023-03-21","","","","","","","","","","","","","","","","","","","<8","","250","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","亚硝酸盐","2023-03-21","","","","","","","","","","","","","","","","","","","0.004","","1.00","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","不评价(/)","废水","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","粪大肠菌群","2023-03-21","","","","","","","","","","","","","","","","","","","600","","","","MPN/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","氰化物","2023-03-21","","","","","","","","","","","","","","","","","","","<0.004","","0.05","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","铜","2023-03-21","","","","","","","","","","","","","","","","","","","<0.05","","1.00","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","镉","2023-03-21","","","","","","","","","","","","","","","","","","","0.0002","","0.005","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","氯化物","2023-03-21","","","","","","","","","","","","","","","","","","","<10","","250","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","汞","2023-03-21","","","","","","","","","","","","","","","","","","","<0.00004","","0.001","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","挥发性酚类（以苯酚计）","2023-03-21","","","","","","","","","","","","","","","","","","","<0.0003","","0.002","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","锌","2023-03-21","","","","","","","","","","","","","","","","","","","<0.05","","1.0","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","砷","2023-03-21","","","","","","","","","","","","","","","","","","","0.0034","","0.01","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","本底井  北纬23°50ˊ34.32〞  东经114°45ˊ56.51〞","耗氧量（COD法，以O2计）","2023-03-21","","","","","","","","","","","","","","","","","","","0.57","","3.0","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","溶解性总固体","2023-03-21","","","","","","","","","","","","","","","","","","","241","","1000","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","pH值","2023-03-21","","","","","","","","","","","","","","","","","","","6.8","","8.5","6.5","无量纲","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","总硬度","2023-03-21","","","","","","","","","","","","","","","","","","","<5","","450","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","铬（六价）","2023-03-21","","","","","","","","","","","","","","","","","","","<0.004","","0.05","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","砷","2023-03-21","","","","","","","","","","","","","","","","","","","0.0009","","0.01","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","锰","2023-03-21","","","","","","","","","","","","","","","","","","","<0.01","","0.10","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","硝酸盐（以N计）","2023-03-21","","","","","","","","","","","","","","","","","","","0.99","","20.0","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","不评价(/)","废水","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","粪大肠菌群","2023-03-21","","","","","","","","","","","","","","","","","","","13000","","","","MPN/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","汞","2023-03-21","","","","","","","","","","","","","","","","","","","<0.00004","","0.001","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","耗氧量（COD法，以O2计）","2023-03-21","","","","","","","","","","","","","","","","","","","1.02","","3.0","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","锌","2023-03-21","","","","","","","","","","","","","","","","","","","<0.05","","1.0","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","挥发性酚类（以苯酚计）","2023-03-21","","","","","","","","","","","","","","","","","","","<0.0003","","0.002","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","铜","2023-03-21","","","","","","","","","","","","","","","","","","","<0.05","","1.00","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","铅","2023-03-21","","","","","","","","","","","","","","","","","","","<0.001","","0.01","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","氨氮","2023-03-21","","","","","","","","","","","","","","","","","","","0.542","","0.5","","mg/L","是","0.08",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","氰化物","2023-03-21","","","","","","","","","","","","","","","","","","","<0.004","","0.05","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","铁","2023-03-21","","","","","","","","","","","","","","","","","","","<0.03","","0.3","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","镉","2023-03-21","","","","","","","","","","","","","","","","","","","0.0002","","0.005","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","氟化物","2023-03-21","","","","","","","","","","","","","","","","","","","0.64","","1.0","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","氯化物","2023-03-21","","","","","","","","","","","","","","","","","","","<10","","250","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","硫酸盐","2023-03-21","","","","","","","","","","","","","","","","","","","<8","","250","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井2 北纬23°50ˊ29.09〞  东经114°46ˊ3.62〞","亚硝酸盐","2023-03-21","","","","","","","","","","","","","","","","","","","<0.003","","1.00","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","硫酸盐","2023-03-21","","","","","","","","","","","","","","","","","","","<8","","250","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","镉","2023-03-21","","","","","","","","","","","","","","","","","","","0.0003","","0.005","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","锰","2023-03-21","","","","","","","","","","","","","","","","","","","<0.01","","0.10","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","不评价(/)","废水","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","粪大肠菌群","2023-03-21","","","","","","","","","","","","","","","","","","","800","","","","MPN/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","溶解性总固体","2023-03-21","","","","","","","","","","","","","","","","","","","181","","1000","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","砷","2023-03-21","","","","","","","","","","","","","","","","","","","0.0009","","0.01","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","挥发性酚类（以苯酚计）","2023-03-21","","","","","","","","","","","","","","","","","","","<0.0003","","0.002","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","汞","2023-03-21","","","","","","","","","","","","","","","","","","","<0.00004","","0.001","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","氰化物","2023-03-21","","","","","","","","","","","","","","","","","","","<0.004","","0.05","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","总硬度","2023-03-21","","","","","","","","","","","","","","","","","","","<5","","450","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","铅","2023-03-21","","","","","","","","","","","","","","","","","","","<0.001","","0.01","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","锌","2023-03-21","","","","","","","","","","","","","","","","","","","<0.05","","1.0","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","亚硝酸盐","2023-03-21","","","","","","","","","","","","","","","","","","","<0.003","","1.00","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","铜","2023-03-21","","","","","","","","","","","","","","","","","","","<0.05","","1.00","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","氯化物","2023-03-21","","","","","","","","","","","","","","","","","","","<10","","250","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","硝酸盐（以N计）","2023-03-21","","","","","","","","","","","","","","","","","","","0.21","","20.0","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","耗氧量（COD法，以O2计）","2023-03-21","","","","","","","","","","","","","","","","","","","0.81","","3.0","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","pH值","2023-03-21","","","","","","","","","","","","","","","","","","","7.0","","8.5","6.5","无量纲","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","铁","2023-03-21","","","","","","","","","","","","","","","","","","","<0.03","","0.3","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","氨氮","2023-03-21","","","","","","","","","","","","","","","","","","","0.278","","0.5","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","氟化物","2023-03-21","","","","","","","","","","","","","","","","","","","0.51","","1.0","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染扩散井1 北纬23°50ˊ33.40〞  东经114°46ˊ0.55〞","铬（六价）","2023-03-21","","","","","","","","","","","","","","","","","","","<0.004","","0.05","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","耗氧量（COD法，以O2计）","2023-03-21","","","","","","","","","","","","","","","","","","","0.96","","3.0","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","挥发性酚类（以苯酚计）","2023-03-21","","","","","","","","","","","","","","","","","","","<0.0003","","0.002","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","锌","2023-03-21","","","","","","","","","","","","","","","","","","","<0.05","","1.0","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","汞","2023-03-21","","","","","","","","","","","","","","","","","","","<0.00004","","0.001","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","硝酸盐（以N计）","2023-03-21","","","","","","","","","","","","","","","","","","","0.13","","20.0","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","铁","2023-03-21","","","","","","","","","","","","","","","","","","","<0.03","","0.3","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","砷","2023-03-21","","","","","","","","","","","","","","","","","","","0.0008","","0.01","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","氟化物","2023-03-21","","","","","","","","","","","","","","","","","","","0.64","","1.0","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","亚硝酸盐","2023-03-21","","","","","","","","","","","","","","","","","","","0.003","","1.00","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","铜","2023-03-21","","","","","","","","","","","","","","","","","","","<0.05","","1.00","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","不评价(/)","废水","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","粪大肠菌群","2023-03-21","","","","","","","","","","","","","","","","","","","400","","","","MPN/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","pH值","2023-03-21","","","","","","","","","","","","","","","","","","","7.1","","8.5","6.5","无量纲","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","铅","2023-03-21","","","","","","","","","","","","","","","","","","","<0.001","","0.01","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","铬（六价）","2023-03-21","","","","","","","","","","","","","","","","","","","<0.004","","0.05","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","氨氮","2023-03-21","","","","","","","","","","","","","","","","","","","0.797","","0.5","","mg/L","是","0.59",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","氯化物","2023-03-21","","","","","","","","","","","","","","","","","","","<10","","250","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","总硬度","2023-03-21","","","","","","","","","","","","","","","","","","","<5","","450","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","溶解性总固体","2023-03-21","","","","","","","","","","","","","","","","","","","233","","1000","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","锰","2023-03-21","","","","","","","","","","","","","","","","","","","<0.01","","0.10","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","氰化物","2023-03-21","","","","","","","","","","","","","","","","","","","<0.004","","0.05","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","硫酸盐","2023-03-21","","","","","","","","","","","","","","","","","","","<8","","250","","mg/L","否","",""]
["2023年东源县第一季度垃圾处理企业和污染源监测","东源县仙塘镇生活垃圾卫生填埋场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","污染监视井1 北纬23°50ˊ31.93〞  东经114°46ˊ3.13〞","镉","2023-03-21","","","","","","","","","","","","","","","","","","","0.0004","","0.005","","mg/L","否","",""]