{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["废水排放","无组织","周边环境"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"废水排放","index":0,"n_rows":35,"n_cols":22,"rows_kept":35,"merged":[[1,0,19,0],[1,1,19,1],[20,0,34,0],[20,1,34,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","受纳水体","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","流量(m³/s)","水温(°C)","生产负荷(%)","进口浓度","排放浓度","上限","下限","单位","是否超标","超标倍数","备注","是否有评价限值"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,2005年12月31日前建设","出水口","总磷（以P计）","2023-03-20","","","","","0.69","1","","mg/L","否","","","是"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","出水口","化学需氧量","2023-03-20","","","","","20","40","","mg/L","否","","","是"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","出水口","悬浮物","2023-03-20","","","","","8","20","","mg/L","否","","","是"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","出水口","石油类","2023-03-20","","","","","<0.06","3","","mg/L","否","","","是"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","出水口","动植物油","2023-03-20","","","","","<0.06","3","","mg/L","否","","","是"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","出水口","氨氮（NH3-N）","2023-03-20","","","","","5.80","8;15","","mg/L","否","","","是"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","出水口","色度","2023-03-20","","","","","0","30","","倍","否","","","是"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","出水口","阴离子表面活性剂（LAS）","2023-03-20","","","","","0.100","1","","mg/L","否","","","是"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","出水口","粪大肠菌群数","2023-03-20","","","","","438","10000","","个/L","否","","","是"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","出水口","pH值","2023-03-20","","","","","7.00","9","6","无量纲","否","","","是"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","出水口","总氮（以N计）","2023-03-20","","","","","15.08","20","","mg/L","否","","","是"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","出水口","五日生化需氧量","2023-03-20","","","","","7.9","20","","mg/L","否","","","是"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","出水口","总镉","2023-03-20","","","","","<0.001","0.01","","mg/L","否","","","是"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","出水口","总汞","2023-03-20","","","","","0.00015","0.001","","mg/L","否","","","是"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","出水口","烷基汞","2023-03-20","","","","","<10","0","","mg/L","否","","","是"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","出水口","六价铬","2023-03-20","","","","","<0.004","0.05","","mg/L","否","","","是"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","出水口","总砷","2023-03-20","","","","","0.0082","0.1","","mg/L","否","","","是"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","出水口","总铅","2023-03-20","","","","","<0.01","0.1","","mg/L","否","","","是"]
["2023年紫金县城区污水处理厂第1季度","紫金县城区污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","出水口","总铬","2023-03-20","","","","","0.029","0.1","","mg/L","否","","","是"]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(DW001)","总汞","2023-02-14","","","","","<0.00004","0.001","","mg/L","否","","","是"]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(DW001)","悬浮物","2023-02-14","","","","","7","10","","mg/L","否","","","是"]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(DW001)","总砷","2023-02-14","","","","","<0.0003","0.1","","mg/L","否","","","是"]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(DW001)","总氮（以N计）","2023-02-14","","","","","8.54","15","","mg/L","否","","","是"]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","排放口(DW001)","总磷（以P计）","2023-02-14","","","","","0.02","0.5","","mg/L","否","","","是"]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(DW001)","总铅","2023-02-14","","","","","0.002","0.1","","mg/L","否","","","是"]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(DW001)","氨氮（NH3-N）","2023-02-14","","","","","2.46","5","","mg/L","否","","","是"]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(DW001)","pH值","2023-02-14","","","","","7.1","9","6","无量纲","否","","","是"]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(DW001)","五日生化需氧量","2023-02-14","","","","","4.0","10","","mg/L","否","","","是"]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(DW001)","粪大肠菌群数","2023-02-14","","","","","<20","1000","","个/L","否","","","是"]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(DW001)","总镉","2023-02-14","","","","","<0.0001","0.01","","mg/L","否","","","是"]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(DW001)","化学需氧量","2023-02-14","","","","","17","50","","mg/L","否","","","是"]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(DW001)","六价铬","2023-02-14","","","","","<0.004","0.05","","mg/L","否","","","是"]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(DW001)","色度","2023-02-14","","","","","2","30","","倍","否","","","是"]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(DW001)","总铬","2023-02-14","","","","","0.011","0.1","","mg/L","否","","","是"]

{"sheet":"无组织","index":1,"n_rows":3,"n_cols":20,"rows_kept":3,"merged":[[1,0,2,0],[1,1,2,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","风向","风速（m/s）","温度(℃)","压力（kPa）","排放浓度","上限","下限","单位","是否超标","超标倍数","备注"]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","不评价的项目（新疆）(DB001XJ)","废气项目","2#下风向","甲烷","2023-02-14","","","","","0.000259","","","mg/m3","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","2#下风向","臭气浓度","2023-02-14","","","","","13","20","","无量纲","否","",""]

{"sheet":"周边环境","index":2,"n_rows":24,"n_cols":35,"rows_kept":24,"merged":[[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,0,13],[0,14,0,17],[0,18,0,19],[0,20,0,24],[0,25,0,26],[0,27,1,27],[0,28,1,28],[0,29,1,29],[0,30,1,30],[0,31,1,31],[0,32,1,32],[0,33,1,33],[0,34,1,34],[2,0,23,0],[2,1,23,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","周边环境-环境空气","周边环境-环境空气","周边环境-环境空气","周边环境-环境空气","周边环境-环境空气","周边环境-地表水","周边环境-地表水","周边环境-地表水","周边环境-地表水","周边环境-地下水","周边环境-地下水","周边环境-土壤","周边环境-土壤","周边环境-土壤","周边环境-土壤","周边环境-土壤","周边环境-噪声","周边环境-噪声","折算/浓度/昼间","夜间","上限","下限","单位","是否超标","超标倍数","备注"]
["","","","","","","","","","湿度(%)","气温（℃","气压(kPa)","风速(m/s)","风向","流量(m³/s)","感官描述","有无漂浮物","有无油","井深（m）","水位（m）","采样深度(m)","土壤颜色","土壤水分(%)","利用情况","土壤pH值","声源","风速(m/s)","","","","","","","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","pH值","2023-02-14","","","","","","","","","","","","","","","","","","","7.0","","8.5","6.5","无量纲","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","氯化物","2023-02-14","","","","","","","","","","","","","","","","","","","3.46","","250","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","硝酸盐（以N计）","2023-02-14","","","","","","","","","","","","","","","","","","","1.11","","20.0","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","铜","2023-02-14","","","","","","","","","","","","","","","","","","","0.00149","","1.00","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","氰化物","2023-02-14","","","","","","","","","","","","","","","","","","","<0.004","","0.05","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","氟化物","2023-02-14","","","","","","","","","","","","","","","","","","","0.226","","1.0","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","锰","2023-02-14","","","","","","","","","","","","","","","","","","","0.00024","","0.10","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","锌","2023-02-14","","","","","","","","","","","","","","","","","","","0.0118","","1.0","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","铅","2023-02-14","","","","","","","","","","","","","","","","","","","<0.00009","","0.01","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","铬（六价）","2023-02-14","","","","","","","","","","","","","","","","","","","<0.004","","0.05","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","氨氮","2023-02-14","","","","","","","","","","","","","","","","","","","0.052","","0.5","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","耗氧量（COD法，以O2计）","2023-02-14","","","","","","","","","","","","","","","","","","","1.12","","3.0","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","硫酸盐","2023-02-14","","","","","","","","","","","","","","","","","","","2.10","","250","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","砷","2023-02-14","","","","","","","","","","","","","","","","","","","<0.0003","","0.01","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","挥发性酚类（以苯酚计）","2023-02-14","","","","","","","","","","","","","","","","","","","0.0004","","0.002","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","不评价的项目（新疆）(DB001XJ)","废水项目","地下水1#取水点","粪大肠菌群","2023-02-14","","","","","","","","","","","","","","","","","","","<20","","","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","总硬度","2023-02-14","","","","","","","","","","","","","","","","","","","13.6","","450","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","亚硝酸盐","2023-02-14","","","","","","","","","","","","","","","","","","","<0.016","","1.00","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","铁","2023-02-14","","","","","","","","","","","","","","","","","","","0.00252","","0.3","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","溶解性总固体","2023-02-14","","","","","","","","","","","","","","","","","","","30","","1000","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","镉","2023-02-14","","","","","","","","","","","","","","","","","","","<0.00005","","0.005","","mg/L","否","",""]
["2023紫金县生活垃圾卫生填埋场第1季度","紫金县城区生活垃圾无害化处理场","土壤环境","环境卫生管理","地下水质量标准(GB/T 14848-2017)","（表1）地下水质量常规指标及限值,Ⅲ类","地下水1#取水点","汞","2023-02-14","","","","","","","","","","","","","","","","","","","<0.00004","","0.001","","mg/L","否","",""]